-- Diese Version ist für Linux (x86 - deb) 
Version 0.1.0 (beta)

Dieser Installationsprozess bezieht sich ausschließlich auf die Beta Version von SMARTfloor Connect


1. Den gesamten Ordner "SMARTfloorConnect_deb" in Dokumente oder einen ähnlichen Ordner kopieren
2. Die Datei ausführbar machen: sudo chmod +x smartfloor-connect-app
3. Es müssen noch Berechtigungen zur Kommunikation mit dem USB Empfänger gesetzt werden.

Option 1:

sudo usermod -aG dialout $USER

Dann abmelden und wieder anmelden (oder newgrp dialout).


Falls das nicht funktioniert:

Option 2:

sudo chmod 666 /dev/{USB PORT} (meist ttyUSB0, ttyUSB1 etc...)


ACHTUNG es kann zu Problemen unter Wayland kommen. Falls keine Tastatureingabe erfolgt, bitte zu X11 wechseln.





-- This version is for Linux (x86 - deb) 
Version 0.1.0 (beta)

This installation process applies exclusively to the beta version of SMARTfloor Connect


1. Copy the entire ‘SMARTfloorConnect_deb’ folder to Documents or a similar folder
2. Make the file executable: sudo chmod +x smartfloor-connect-app
3. Permissions for communication with the USB receiver must still be set.

Option 1:

sudo usermod -aG dialout $USER

Then log out and log back in (or newgrp dialout).


If that does not work:

Option 2:

sudo chmod 666 /dev/{USB PORT} (usually ttyUSB0, ttyUSB1 etc...)


ATTENTION: problems may occur under Wayland. If no keyboard input is possible, please switch to X11.